SAFETY DATA SHEET
DOW AGROSCIENCES S.A.S.

Product name: TELONE™ II Soil Fumigant	Issue Date: 07/10/2018Print Date: 07/10/2018	
DOW AGROSCIENCES S.A.S. encourages you and expects you to read and understand the entire SDS as there is important information throughout the document. This SDS provides users with information relating to the protection of human health and safety at the workplace, protection of the environment and supports emergency response. Product users and applicators should primarily refer to the product label attached to or accompanying the product container.

1. PRODUCT AND COMPANY IDENTIFICATION
Product name: TELONE™ II Soil Fumigant

Recommended use of the chemical and restrictions on use
Identified uses: Plant Protection Product active substance  

COMPANY IDENTIFICATION
DOW AGROSCIENCES S.A.S.
371, RUE LUDWIG VAN BEETHOVEN
06560 VALBONNE
FRANCE

Customer Information Number:(0) 493 95 60 00
SDSQuestion@dow.com
Emergency telephone number
24-Hour Emergency Contact: 0033 388 736 000
Local Emergency Contact: 00 31 115 69 4982

2. HAZARDS IDENTIFICATION

Classification of the substance or mixture
Flammable liquids - Category 3 - H226
Acute toxicity - Category 3 - Oral - H301
Acute toxicity - Category 3 - dermal - H311
Acute toxicity - Category 3 - Inhalation - H331
Eye irritation - Category 2 - H319
Skin irritation - Category 2 - H315
Skin sensitisation - Category 1 - H317
Aspiration hazard - Category 1 - H304
Specific target organ toxicity - single exposure - Category 3 - Inhalation - H335
Acute aquatic toxicity - Category 1 - H400
Chronic aquatic toxicity - Category 1 - H410
For the full text of the H-Statements mentioned in this Section, see Section 16.

Label elements

Hazard pictograms

Signal word: Danger

Hazard statements
H226	Flammable liquid and vapour.	H301	Toxic if swallowed.	H311	Toxic in contact with skin.	H331	Toxic if inhaled.	H315	Causes skin irritation.	H319	Causes serious eye irritation.	H317	May cause an allergic skin reaction.	H335	May cause respiratory irritation.	H304	May be fatal if swallowed and enters airways.	H410	Very toxic to aquatic life with long lasting effects.	
Precautionary statements
P261	Avoid breathing mist or vapours.	P280	Wear protective gloves/ protective clothing/ eye protection/ face protection.	P304 + P340	IF INHALED: Remove victim to fresh air and keep at rest in a position comfortable for breathing.	P308 + P311	IF exposed or concerned: Call a POISON CENTER/doctor.	P405	Store locked up.	P501	Dispose of contents/container in accordance with applicable regulations.	
Supplemental information
EUH401	To avoid risks to human health and the environment, comply with the instructions for use.			

Other hazards
No data available
3. COMPOSITION/INFORMATION ON INGREDIENTS

This product is a substance.
CASRN / 
EC-No. / 
Index-No.Concentration	Component	Classification	CASRN
542-75-6
EC-No.
208-826-5
Index-No.
602-030-00-5	97.5%	1,3-Dichloropropene	Flam. Liq. - 3 - H226
Acute Tox. - 3 - H301
Acute Tox. - 3 - H331
Acute Tox. - 3 - H311
Skin Irrit. - 2 - H315
Eye Irrit. - 2 - H319
Skin Sens. - 1 - H317
STOT SE - 3 - H335
Asp. Tox. - 1 - H304
Aquatic Acute - 1 - H400
Aquatic Chronic - 1 - H410
	For the full text of the H-Statements mentioned in this Section, see Section 16.

4. FIRST AID MEASURES
Description of first aid measures
General advice: First Aid responders should pay attention to self-protection and use the recommended protective clothing (chemical resistant gloves, splash protection).  If potential for exposure exists refer to Section 8 for specific personal protective equipment.  

Inhalation: Move person to fresh air. If person is not breathing, call an emergency responder or ambulance, then give artificial respiration; if by mouth to mouth use rescuer protection (pocket mask etc). Call a poison control center or doctor for treatment advice.  If breathing is difficult, oxygen should be administered by qualified personnel.  

Skin contact: Take off contaminated clothing. Wash skin with soap and plenty of water for 15-20 minutes. Call a poison control center or doctor for treatment advice.  Wash clothing before reuse. Shoes and other leather items which cannot be decontaminated should be disposed of properly.  Suitable emergency safety shower facility should be immediately available.  

Eye contact: Hold eyes open and rinse slowly and gently with water for 15-20 minutes. Remove contact lenses, if present, after the first 5 minutes, then continue rinsing eyes. Call a poison control center or doctor for treatment advice.  Suitable emergency eye wash facility should be immediately available.  

Ingestion: Seek medical attention immediately.  Do not induce vomiting. Call a physician and/or transport to emergency facility immediately.  

Most important symptoms and effects, both acute and delayed: 
Aside from the information found under Description of first aid measures (above) and Indication of immediate medical attention and special treatment needed (below), any additional important symptoms and effects are described in Section 11: Toxicology Information.

Indication of any immediate medical attention and special treatment needed
Notes to physician: Skin contact may aggravate preexisting dermatitis.  Maintain adequate ventilation and oxygenation of the patient.  May cause asthma-like (reactive airways) symptoms.  Bronchodilators, expectorants, antitussives and corticosteroids may be of help.  Respiratory symptoms, including pulmonary edema, may be delayed. Persons receiving significant exposure should be observed 24-48 hours for signs of respiratory distress.  Because rapid absorption may occur through the lungs if aspirated and cause systemic effects, the decision of whether to induce vomiting or not should be made by a physician.  If lavage is performed, suggest endotracheal and/or esophageal control.  Danger from lung aspiration must be weighed against toxicity when considering emptying the stomach.  Animal data indicates that this material is a potential skin sensitizer. However, skin sensitization has not been encountered among employees involved in the manufacture of this material.  No specific antidote.  Treatment of exposure should be directed at the control of symptoms and the clinical condition of the patient.  Have the Safety Data Sheet, and if available, the product container or label with you when calling a poison control center or doctor, or going for treatment.  

5. FIREFIGHTING MEASURES
Suitable extinguishing media: Water fog or fine spray.  Dry chemical fire extinguishers.  Carbon dioxide fire extinguishers.  Foam.  General purpose synthetic foams (including AFFF type) or protein foams are preferred if available.  Alcohol resistant foams (ATC type) may function.  Water fog, applied gently may be used as a blanket for fire extinguishment.  

Unsuitable extinguishing media: Do not use direct water stream.  Straight or direct water streams may not be effective to extinguish fire.  

Special hazards arising from the substance or mixture
Hazardous combustion products: During a fire, smoke may contain the original material in addition to combustion products of varying composition which may be toxic and/or irritating.  Combustion products may include and are not limited to:  Hydrogen chloride.  Carbon monoxide.  Carbon dioxide.  

Unusual Fire and Explosion Hazards:   Container may rupture from gas generation in a fire situation.  Electrically ground and bond all equipment.  Flammable mixtures of this product are readily ignited even by static discharge.  Vapors are heavier than air and may travel a long distance and accumulate in low lying areas. Ignition and/or flash back may occur.  Flammable mixtures may exist within the vapor space of containers at room temperature.  Flammable concentrations of vapor can accumulate at temperatures above flash point; see Section 9.  

Advice for firefighters
Fire Fighting Procedures: Keep people away.  Isolate fire and deny unnecessary entry.  Stay upwind. Keep out of low areas where gases (fumes) can accumulate.  Water may not be effective in extinguishing fire.  Use water spray to cool fire exposed containers and fire affected zone until fire is out and danger of reignition has passed.  Fight fire from protected location or safe distance. Consider the use of unmanned hose holders or monitor nozzles.  Immediately withdraw all personnel from the area in case of rising sound from venting safety device or discoloration of the container.  Do not use direct water stream. May spread fire.  Eliminate ignition sources.  Move container from fire area if this is possible without hazard.  Burning liquids may be moved by flushing with water to protect personnel and minimize property damage.  Water fog, applied gently may be used as a blanket for fire extinguishment.  Contain fire water run-off if possible. Fire water run-off, if not contained, may cause environmental damage.  Review the "Accidental Release Measures" and the "Ecological Information" sections of this (M)SDS.  

Special protective equipment for firefighters: Wear positive-pressure self-contained breathing apparatus (SCBA) and protective fire fighting clothing (includes fire fighting helmet, coat, trousers, boots, and gloves).  Avoid contact with this material during fire fighting operations. If contact is likely, change to full chemical resistant fire fighting clothing with self-contained breathing apparatus.  If this is not available, wear full chemical resistant clothing with self-contained breathing apparatus and fight fire from a remote location.  For protective equipment in post-fire or non-fire clean-up situations, refer to the relevant sections.  

6. ACCIDENTAL RELEASE MEASURES
Personal precautions, protective equipment and emergency procedures: Isolate area.  Keep unnecessary and unprotected personnel from entering the area.  Refer to section 7, Handling, for additional precautionary measures.  Keep personnel out of low areas.  Keep upwind of spill.  Ventilate area of leak or spill.  No smoking in area.  Eliminate all sources of ignition in vicinity of spill or released vapor to avoid fire or explosion.  Vapor explosion hazard. Keep out of sewers.  For large spills, warn public of downwind explosion hazard.  Check area with combustible gas detector before reentering area. Ground and bond all containers and handling equipment.  Use appropriate safety equipment. For additional information, refer to Section 8, Exposure Controls and Personal Protection.  

Environmental precautions: Prevent from entering into soil, ditches, sewers, waterways and/or groundwater. See Section 12, Ecological Information.  Spills or discharge to natural waterways is likely to kill aquatic organisms.  

Methods and materials for containment and cleaning up: Ground and bond all containers and handling equipment.  Pump with explosion-proof equipment. If available, use foam to smother or suppress.  Contain spilled material if possible.  Small spills:  Absorb with materials such as:  Clay.  Dirt.  Sand.  Sweep up.  Collect in suitable and properly labeled containers.  Large spills:  Contact Dow AgroSciences for clean-up assistance.  See Section 13, Disposal Considerations, for additional information.  

7. Handling and storage
Precautions for safe handling: Keep out of reach of children.  Keep away from heat, sparks and flame.  Electrically bond and ground all containers, personnel and equipment before transfer or use of material.  Vapors are heavier than air and may travel a long distance and accumulate in low lying areas. Ignition and/or flash back may occur.  Avoid contact with eyes, skin, and clothing.  Avoid breathing vapor or mist.  Do not swallow.  Wash thoroughly after handling.  Keep container closed.  Use only with adequate ventilation.  Never use air pressure for transferring product.  No smoking, open flames or sources of ignition in handling and storage area.  Containers, even those that have been emptied, can contain vapors. Do not cut, drill, grind, weld, or perform similar operations on or near empty containers.  Use of non-sparking or explosion-proof equipment may be necessary, depending upon the type of operation.  See Section 8, EXPOSURE CONTROLS AND PERSONAL PROTECTION.  

Conditions for safe storage: Minimize sources of ignition, such as static build-up, heat, spark or flame.  Keep container closed.  Do not store in:  Zinc.  Aluminum.  Aluminum alloys.  Magnesium.  Magnesium alloys.  Flammable mixtures may exist within the vapor space of containers at room temperature.  Store in a dry place.  Store in original container.  Keep container tightly closed.  Do not store near food, foodstuffs, drugs or potable water supplies.  

8. EXPOSURE CONTROLS/PERSONAL PROTECTION
Control parameters
If exposure limits exist, they are listed below.  If no exposure limits are displayed, then no values are applicable.
Component	Regulation	Type of listing	Value/Notation	1,3-Dichloropropene	ACGIH	TWA 	  1 ppm		ACGIH	TWA 	   SKIN	
RECOMMENDATIONS IN THIS SECTION ARE FOR MANUFACTURING, COMMERCIAL BLENDING AND PACKAGING WORKERS. APPLICATORS AND HANDLERS SHOULD SEE THE PRODUCT LABEL FOR PROPER PERSONAL PROTECTIVE EQUIPMENT AND CLOTHING.  

Exposure controls
Engineering controls: Use engineering controls to maintain airborne level below exposure limit requirements or guidelines.  If there are no applicable exposure limit requirements or guidelines, use only with adequate ventilation.  Local exhaust ventilation may be necessary for some operations.  

Individual protection measures
Eye/face protection: Use chemical goggles.  Chemical goggles should be consistent with EN 166 or equivalent.  If exposure causes eye discomfort, use a full-face respirator.  
Skin protection
Hand protection: Use chemical resistant gloves classified under Standard EN374: Protective gloves against chemicals and micro-organisms.  Examples of preferred glove barrier materials include:  Ethyl vinyl alcohol laminate ("EVAL").  Viton.  Examples of acceptable glove barrier materials include:  Neoprene.  Nitrile/butadiene rubber ("nitrile" or "NBR").  When prolonged or frequently repeated contact may occur, a glove with a protection class of 5 or higher (breakthrough time greater than 240 minutes according to EN 374) is recommended.  When only brief contact is expected, a glove with a protection class of 1 or higher (breakthrough time greater than 10 minutes according to EN 374) is recommended.  NOTICE: The selection of a specific glove for a particular application and duration of use in a workplace should also take into account all relevant workplace factors such as, but not limited to: Other chemicals which may be handled, physical requirements (cut/puncture protection, dexterity, thermal protection), potential body reactions to glove materials, as well as the instructions/specifications provided by the glove supplier.  
Other protection: Use protective clothing chemically resistant to this material.  Selection of specific items such as face shield, boots, apron, or full body suit will depend on the task.  
Respiratory protection: Respiratory protection should be worn when there is a potential to exceed the exposure limit requirements or guidelines.  If there are no applicable exposure limit requirements or guidelines, use an approved respirator.  Selection of air-purifying or positive-pressure supplied-air will depend on the specific operation and the potential airborne concentration of the material.  For emergency conditions, use an approved positive-pressure self-contained breathing apparatus.  
Use the following CE approved air-purifying respirator:  Organic vapor cartridge with a particulate pre-filter, type AP2.  

See SECTION 7: Handling and storage and SECTION 13: Disposal considerations for measures to prevent excessive environmental exposure during use and waste disposal.

9. PHYSICAL AND CHEMICAL PROPERTIES
Appearance
Physical state	Liquid.  	ColorColorless to yellow  Odor	Sweet  	Odor Threshold	No test data available  	pH	6.5   1% CIPAC MT 75 (1% aqueous suspension)Melting point/range	Not applicableFreezing point	No test data availableBoiling point (760 mmHg)	107 °C Flash point	closed cup 27 °C EC Method A9 Evaporation Rate (Butyl Acetate = 1)	No test data availableFlammability (solid, gas)	Not applicable to liquids  Lower explosion limit	No test data available  Upper explosion limit	No test data available  Vapor Pressure	23 mmHg  at 20 °C Relative Vapor Density (air = 1)	3.8  	Relative Density (water = 1)	1.21  at 20 °C  / 4 °C  Pyknometer 	Water solubility	Insoluble  	Partition coefficient: n-octanol/water	log Pow: 1.82 - 2.1 Measured 	Auto-ignition temperature	92/69/EEC A15  none below 400 degC  	Decomposition temperature	No test data available  	Dynamic Viscosity	0.66 mPa.s at 40 °C 	Kinematic Viscosity	0.636 mm2/s at 20 °C 	Explosive properties	No 	Oxidizing properties	No 	Liquid Density	1.211 g/cm3 at 20 °C Digital density meter 	Molecular weight	No data available	
NOTE:  The physical data presented above are typical values and should not be construed as a specification.
10. STABILITY AND REACTIVITY
Reactivity: No dangerous reaction known under conditions of normal use.  

Chemical stability: Unstable at elevated temperatures.  

Possibility of hazardous reactions: Polymerization will not occur.  
 
Conditions to avoid: Exposure to elevated temperatures can cause product to decompose.  Generation of gas during decomposition can cause pressure in closed systems.  Avoid static discharge.  

Incompatible materials: Avoid contact with:  Acids.  Bases.  Oxidizers.  Avoid contact with metals such as:  Zinc.  Cadmium.  Magnesium.  Aluminum.  Aluminum alloys.  

Hazardous decomposition products:  Decomposition products depend upon temperature, air supply and the presence of other materials.  Decomposition products can include and are not limited to:  Carbon monoxide.  Carbon dioxide.  Hydrogen chloride.  Toxic gases are released during decomposition.  Decomposition products can include trace amounts of:  Phosgene.  
11. TOXICOLOGICAL INFORMATION

Toxicological information appears in this section when such data is available. 

Acute toxicity
Acute oral toxicity
Moderate toxicity if swallowed.  Small amounts swallowed incidentally as a result of normal handling operations are not likely to cause injury; however, swallowing larger amounts may cause injury.  Swallowing may result in gastrointestinal irritation.  

LD50. Rat. > 110 mg/kg  

Acute dermal toxicity
Prolonged or widespread skin contact may result in absorption of harmful amounts.  

LD50. Rabbit. 333 mg/kg 

Acute inhalation toxicity
Prolonged excessive exposure may cause serious adverse effects, even death.  Excessive exposure may cause irritation to upper respiratory tract (nose and throat) and lungs.  Observations in animals include:  Lethargy.  

LC50. Rat. 4 Hour. vapour. > 2.7 - < 3.07 mg/l 

Skin corrosion/irritation
Brief contact may cause moderate skin irritation with local redness.
May cause drying and flaking of the skin.

Serious eye damage/eye irritation
May cause severe eye irritation.
May cause slight corneal injury.
Vapor may cause lacrimation (tears).
Vapor may cause eye irritation experienced as mild discomfort and redness.

Sensitization
Animal data indicate that 1,3-dichloropropene is a potential skin sensitizer.

For respiratory sensitization:
No relevant data found.

Specific Target Organ Systemic Toxicity (Single Exposure)
May cause respiratory irritation.

Specific Target Organ Systemic Toxicity (Repeated Exposure)
In animals, effects have been reported on the following organs:
Bladder.
Nasal tissue.
Liver.
Lung.
Gastrointestinal tract.
Respiratory tract.
Blood-forming organs (Bone marrow & Spleen).

Carcinogenicity
Has been shown to cause cancer in laboratory animals by the oral route.  Inhalation exposure resulted in an increase in the normal occurrence of benign lung tumors in male mice.  

Teratogenicity
Did not cause birth defects or other effects in the fetus even at doses which caused toxic effects in the mother.  

Reproductive toxicity
In animal studies, did not interfere with reproduction.  

Mutagenicity
In vitro genetic toxicity studies were negative in some cases and positive in other cases.  Animal genetic toxicity studies were negative.  

Aspiration Hazard
May be fatal if swallowed and enters airways.  

12. ECOLOGICAL INFORMATION

Ecotoxicological information appears in this section when such data is available.

Toxicity
Acute toxicity to fish
Material is very toxic to aquatic organisms (LC50/EC50/IC50 below 1 mg/L in the most sensitive species).

LC50. Oncorhynchus mykiss (rainbow trout). 96 Hour. 2.78 mg/l

LC50. Cyprinodon variegatus (sheepshead minnow). 96 Hour. 0.87 mg/l

LC50. Lepomis macrochirus (Bluegill sunfish). 96 Hour. 3.7 mg/l

Acute toxicity to aquatic invertebrates
EC50. Daphnia magna (Water flea). 48 Hour. 3.58 mg/l

EC50. eastern oyster (Crassostrea virginica). 48 Hour. 0.64 mg/l

Acute toxicity to algae/aquatic plants
EbC50. Pseudokirchneriella subcapitata (green algae). static test. 72 Hour. Biomass. 14.9 mg/l

EC50. diatom Navicula sp.. 120 Hour. Biomass. 2.35 mg/l

EC50. Lemna gibba. 14 d. 14.56 mg/l

Chronic aquatic toxicity
Chronic toxicity to fish
NOEC. Pimephales promelas (fathead minnow). flow-through test. 33 d. survival. 0.0318 mg/l

Chronic toxicity to aquatic invertebrates
NOEC. Daphnia magna (Water flea). 21 d. number of offspring. 0.0701 mg/l

Toxicity to Above Ground Organisms
Material is moderately toxic to birds on an acute basis (LD50 between 51 and 500 mg/kg).
Material is practically non-toxic to birds on a dietary basis (LC50 > 5000 ppm).

oral LD50. Colinus virginianus (Bobwhite quail). mortality. 139.8mg/kg bodyweight.

dietary LC50. Anas platyrhynchos (Mallard duck). > 6243mg/kg diet.

Toxicity to soil-dwelling organisms
LC50. Eisenia fetida (earthworms). 14 d. 55.6 mg/kg

Persistence and degradability
Biodegradability: Biodegradation may occur under aerobic conditions (in the presence of oxygen).  
10-day Window: Fail  
Biodegradation:  4.9 % 
Method: OECD Test Guideline 301D or Equivalent  

Theoretical Oxygen Demand:  1.281 mg/mg  

Biological oxygen demand (BOD)

Incubation TimeBOD 0.148 mg/mg

Stability in Water (1/2-life)
Hydrolysis. half-life. 2.3 - 4.75 d

Photodegradation
Atmospheric half-life: 7 - 12 Hour

Bioaccumulative potential
Bioaccumulation: No data available for this product.  For similar material(s):  Bioconcentration potential is low (BCF < 100 or Log Pow < 3).  
Partition coefficient: n-octanol/water(log Pow): 1.82 - 2.1 Measured 

Mobility in soil
For similar material(s):
Potential for mobility in soil is very high (Koc between 0 and 50).
Partition coefficient (Koc): 44.7 Measured

Results of PBT and vPvB assessment
This substance is not considered to be persistent, bioaccumulating and toxic (PBT).  This substance is not considered to be very persistent and very bioaccumulating (vPvB).  

Other adverse effects
1,3-Dichloropropene has a stratospheric ozone depletion potential (ODP) of 0.002, relative to CFC 12 (ODP=1).

13. DISPOSAL CONSIDERATIONS
Disposal methods: 
If wastes and/or containers cannot be disposed of according to the product label directions, disposal of this material must be in accordance with your local or area regulatory authorities.  This information presented below only applies to the material as supplied.  The identification based on characteristic(s) or listing may not apply if the material has been used or otherwise contaminated.  It is the responsibility of the waste generator to determine the toxicity and physical properties of the material generated to determine the proper waste identification and disposal methods in compliance with applicable regulations.  If the material as supplied becomes a waste, follow all applicable regional, national and local laws.  

14. TRANSPORT INFORMATION

Classification for ROAD and Rail transport:
Proper shipping name	PESTICIDE, LIQUID, TOXIC, FLAMMABLE, N.O.S.(1,3-Dichloropropene)	UN number	UN  2903	Class	6.1 (3)	Packing group	II	Environmental hazards	1,3-Dichloropropene	

Classification for SEA transport (IMO-IMDG):
Proper shipping name	PESTICIDE, LIQUID, TOXIC, FLAMMABLE, N.O.S.(1,3-Dichloropropene)	UN number	UN  2903	Class	6.1 (3)	Packing group	II	Marine pollutant	1,3-Dichloropropene	Transport in bulk according to Annex I or II of MARPOL 73/78 and the IBC or IGC Code	Consult IMO regulations before transporting ocean bulk	
Classification for AIR transport (IATA/ICAO):
Proper shipping name	Pesticide, liquid, toxic, flammable, n.o.s.(1,3-Dichloropropene)	UN number	UN  2903	Class	6.1 (3)	Packing group	II	

This information is not intended to convey all specific regulatory or operational requirements/information relating to this product.  Transportation classifications may vary by container volume and may be influenced by regional or country variations in regulations.  Additional transportation system information can be obtained through an authorized sales or customer service representative.  It is the responsibility of the transporting organization to follow all applicable laws, regulations and rules relating to the transportation of the material.

15. REGULATORY INFORMATION

Seveso III: Directive 2012/18/EU of the European Parliament and of the Council on the control of major-accident hazards involving dangerous substances.
Listed in Regulation: ACUTE TOXIC
Number in Regulation: H2
50 t
200 t
Listed in Regulation: FLAMMABLE LIQUIDS
Number in Regulation: P5c
5,000 t
50,000 t
Listed in Regulation: ENVIRONMENTAL HAZARDS
Number in Regulation: E1
100 t
200 t

Classification and labeling have been performed according to Regulation (EC) No 1272/2008.
16. OTHER INFORMATION

Full text of H-Statements referred to under sections 2 and 3.
H226Flammable liquid and vapour.	H301Toxic if swallowed.	H304May be fatal if swallowed and enters airways.	H311Toxic in contact with skin.	H315Causes skin irritation.	H317May cause an allergic skin reaction.	H319Causes serious eye irritation.	H331Toxic if inhaled.	H335May cause respiratory irritation.	H400Very toxic to aquatic life.	H410Very toxic to aquatic life with long lasting effects.	
Revision
Identification Number: 99011047 / A285 / Issue Date: 07/10/2018 / Version: 3.0
DAS Code: XRM-5048
Most recent revision(s) are noted by the bold, double bars in left-hand margin throughout this document.

Legend
ACGIH	USA. ACGIH Threshold Limit Values (TLV)	SKIN	Absorbed via skin	TWA	8-hour, time-weighted average	Acute Tox.	Acute toxicity	Aquatic Acute	Acute aquatic toxicity	Aquatic Chronic	Chronic aquatic toxicity	Asp. Tox.	Aspiration hazard	Eye Irrit.	Eye irritation	Flam. Liq.	Flammable liquids	Skin Irrit.	Skin irritation	Skin Sens.	Skin sensitisation	STOT SE	Specific target organ toxicity - single exposure	
Full text of other abbreviations
ADN - European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways; ADR - European Agreement concerning the International Carriage of Dangerous Goods by Road; AICS - Australian Inventory of Chemical Substances; ASTM - American Society for the Testing of Materials; bw - Body weight; CLP - Classification Labelling Packaging Regulation; Regulation (EC) No 1272/2008; CMR - Carcinogen, Mutagen or Reproductive Toxicant; DIN - Standard of the German Institute for Standardisation; DSL - Domestic Substances List (Canada); ECHA - European Chemicals Agency; EC-Number - European Community number; ECx - Concentration associated with x% response; ELx - Loading rate associated with x% response; EmS - Emergency Schedule; ENCS - Existing and New Chemical Substances (Japan); ErCx - Concentration associated with x% growth rate response; GHS - Globally Harmonized System; GLP - Good Laboratory Practice; IARC - International Agency for Research on Cancer; IATA - International Air Transport Association; IBC - International Code for the Construction and Equipment of Ships carrying Dangerous Chemicals in Bulk; IC50 - Half maximal inhibitory concentration; ICAO - International Civil Aviation Organization; IECSC - Inventory of Existing Chemical Substances in China; IMDG - International Maritime Dangerous Goods; IMO - International Maritime Organization; ISHL - Industrial Safety and Health Law (Japan); ISO - International Organisation for Standardization; KECI - Korea Existing Chemicals Inventory; LC50 - Lethal Concentration to 50 % of a test population; LD50 - Lethal Dose to 50% of a test population (Median Lethal Dose); MARPOL - International Convention for the Prevention of Pollution from Ships; n.o.s. - Not Otherwise Specified; NO(A)EC - No Observed (Adverse) Effect Concentration; NO(A)EL - No Observed (Adverse) Effect Level; NOELR - No Observable Effect Loading Rate; NZIoC - New Zealand Inventory of Chemicals; OECD - Organization for Economic Co-operation and Development; OPPTS - Office of Chemical Safety and Pollution Prevention; PBT - Persistent, Bioaccumulative and Toxic substance; PICCS - Philippines Inventory of Chemicals and Chemical Substances; (Q)SAR - (Quantitative) Structure Activity Relationship; REACH - Regulation (EC) No 1907/2006 of the European Parliament and of the Council concerning the Registration, Evaluation, Authorisation and Restriction of Chemicals; RID - Regulations concerning the International Carriage of Dangerous Goods by Rail; SADT - Self-Accelerating Decomposition Temperature; SDS - Safety Data Sheet; SVHC - Substance of very high concern; TCSI - Taiwan Chemical Substance Inventory; TSCA - Toxic Substances Control Act (United States); UN - United Nations; UNRTDG - United Nations Recommendations on the Transport of Dangerous Goods; vPvB - Very Persistent and Very Bioaccumulative

Information Source and References
This SDS is prepared by Product Regulatory Services and Hazard Communications Groups from information supplied by internal references within our company.

DOW AGROSCIENCES S.A.S. urges each customer or recipient of this (M)SDS to study it carefully and consult appropriate expertise, as necessary or appropriate, to become aware of and understand the data contained in this (M)SDS and any hazards associated with the product.  The information herein is provided in good faith and believed to be accurate as of the effective date shown above.  However, no warranty, express or implied, is given.  Regulatory requirements are subject to change and may differ between various locations. It is the buyer's/user's responsibility to ensure that his activities comply with all federal, state, provincial or local laws.  The information presented here pertains only to the product as shipped.  Since conditions for use of the product are not under the control of the manufacturer, it is the buyer's/user's duty to determine the conditions necessary for the safe use of this product.  Due to the proliferation of sources for information such as manufacturer-specific (M)SDSs, we are not and cannot be responsible for (M)SDSs obtained from any source other than ourselves.  If you have obtained an (M)SDS from another source or if you are not sure that the (M)SDS you have is current, please contact us for the most current version.    

IL